NGBE(4) | Device Drivers Manual | NGBE(4)

# NAME

`ngbe` — WangXun WX1860 PCI Express 10/100/1Gb Ethernet device

# SYNOPSIS

`ngbe* at pci?`

# DESCRIPTION

The `ngbe` driver provides support for PCI Express Gigabit Ethernet adapters based on the WangXun WX1860AL1 and WX1860A2 Ethernet controllers, including the following:

- LR-LINK LRES2034PT (WX1860AL1)
- LR-LINK LRES2045PT (WX1860A2)

The `ngbe` driver supports IPv4 receive IP/TCP/UDP checksum offload and VLAN tag insertion and stripping.

The `ngbe` driver supports the following media types:

autoselect
  Enables auto-negotiation for speed and duplex.
10baseT `mediaopt` full-duplex
  Sets 10Mbps operation.
100baseTX `mediaopt` full-duplex
  Sets 100Mbps operation.
1000baseT
  Sets 1000Mbps operation. Only full-duplex mode is supported at this speed.

For more information on configuring this device, see ifconfig(8).

# SEE ALSO

arp(4), ifmedia(4), intro(4), netintro(4), pci(4), hostname.if(5), ifconfig(8)

# HISTORY

The `ngbe` driver first appeared in OpenBSD 7.4.

# AUTHORS

The `ngbe` driver was written by Kevin Lo <kevlo@openbsd.org>.

March 31, 2023 | Debian