LMTEMP(4) | Device Drivers Manual | LMTEMP(4)

# NAME

`lmtemp` — National Semiconductor LM75/LM76/LM77 temperature sensor

# SYNOPSIS

`lmtemp* at iic?`

# DESCRIPTION

The `lmtemp` driver provides support for the National Semiconductor LM75, National Semiconductor LM76, National Semiconductor LM77, Dallas Semiconductor 1775, and Philips Semiconductor LM75A temperature sensors. The sensor possesses a single temperature value that can be accessed through the sysctl(8) interface.

# SEE ALSO

iic(4), intro(4), sensorsd(8), sysctl(8)

# HISTORY

The `lmtemp` driver first appeared in OpenBSD 3.6.

April 15, 2008 | Debian