CLCS(4) | Device Drivers Manual | CLCS(4)

# NAME

`clcs` — Cirrus Logic CS4280/CS4610/CS4615 audio device

# SYNOPSIS

`clcs* at pci?`
`audio* at clcs?`

# DESCRIPTION

The `clcs` driver provides support for the Cirrus Logic CS4280 chip, as well as for CS461x.

# FILES

The driver needs a firmware file, which is loaded on demand when the device is attached:

/etc/firmware/cs4280

# SEE ALSO

ac97(4), audio(4), intro(4), pci(4)

# HISTORY

The `clcs` device driver appeared in OpenBSD 2.8.

June 26, 2008 | Debian