BCMSTBPINCTRL(4) | Device Drivers Manual | BCMSTBPINCTRL(4)

# NAME

`bcmstbpinctrl` — Broadcom Set-top Box pin multiplexing

# SYNOPSIS

`bcmstbpinctrl* at fdt?`

# DESCRIPTION

The `bcmstbpinctrl` driver uses pin control data from the device tree to select one of multiple possible roles available for pins on Broadcom Set-top Box SoCs. This includes the Broadcom BCM2712 SoC that is used in the Raspberry Pi 5. It does not provide direct device driver entry points but makes its functions available to other drivers.

# SEE ALSO

intro(4)

# HISTORY

The `bcmstbpinctrl` driver first appeared in OpenBSD 7.8.

# AUTHORS

The `bcmstbpinctrl` driver was written by Mark Kettenis <kettenis@openbsd.org>.

August 19, 2025 | Debian