RFX(4) | Device Drivers Manual (sparc64) | RFX(4)

# NAME

`rfx` — Vitec/Connectware/AP&D RasterFlex framebuffer series

# SYNOPSIS

`rfx* at sbus?`
`wsdisplay* at rfx?`

# DESCRIPTION

The RasterFlex series, originally manufactured by Vitec, later bought by Connectware, then by Advanced Products & Design, are high-performance frame buffers and frame grabber devices.

The `rfx` driver only supports the RasterFlex frame buffers:

RasterFlex-24
RasterFlex-32
RasterFlex-HR

The `rfx` driver interfaces the frame buffer with the wscons(4) console framework. It does not provide direct device driver entry points but makes its functions available via the internal wsdisplay(4) interface.

# DISPLAY RESOLUTION

The RasterFlex frame buffers will adapt their resolution to the monitor they are connected to. However, when not connected to a Sun monitor, the device will default to the 1152x900 resolution, with a refresh rate of 66Hz. A different resolution can be forced using the jumpers J2 to J4, located near the video connector on the board itself.

In the following tables, left (L) and right (R) jumper positions are described looking at the board with the video connector on top. If the jumper position is not specified (_), it means it has to be removed (open).

## RasterFlex-24 and RasterFlex-32 Jumper Settings:

J2 J3 J4 | Resolution | Refresh Rate | Description
`R R R` | 1152x900 | 66Hz | Automatic Configuration
`L L L` | 1024x768 | 76Hz | SVGA
`L _ _` | 1152x900 | 66Hz |
`_ L L` | 1152x900 | 76Hz |

## RasterFlex-HR Jumper Settings:

J2 J3 J4 | Resolution | Refresh Rate | Description
`R R R` | 1152x900 | 66Hz | Automatic Configuration
`L L L` | 1024x768 | 76Hz | SVGA
`L _ _` | 1152x900 | 66Hz |
`L L _` | 1152x900 | 76Hz |
`_ L _` | 1280x1024 | 60Hz |
`_ L L` | 1280x1024 | 67Hz |
`L _ L` | 1280x1024 | 76Hz |

# SEE ALSO

intro(4), sbus(4), wscons(4), wsdisplay(4)

# CAVEATS

This driver does not support any acceleration features at the moment, and drives the card in PROM-compatible, 8 bit, mode only.

September 10, 2015 | Debian