INTRO(4) | Device Drivers Manual (alpha) | INTRO(4)

# NAME

`intro` — introduction to special files and hardware support

# DESCRIPTION

The manual pages in section 4 describe the special files, related driver functions, and networking support available in the system. In this part of the manual, the SYNOPSIS section of each configurable device gives a sample specification for use in constructing a system description for the config(8) program. The DIAGNOSTICS section lists messages which may appear on the console and/or in the system error log /var/log/messages due to errors in device operation; see syslogd(8) for more information.

This section contains both devices which may be configured into the system and network related information. The networking support is introduced in netintro(4).

# DEVICE SUPPORT

This section describes the hardware supported on the Alpha platform. Software support for these devices comes in two forms. A hardware device may be supported with a character or block device driver, or it may be used within the networking subsystem and have a network interface driver. Block and character devices are accessed through files in the file system of a special type; see mknod(8). Network interfaces are indirectly accessed through the interprocess communication facilities provided by the system; see socket(2).

A hardware device is identified to the system at configuration time and the appropriate device or network interface driver is then compiled into the system. When the resultant system is booted, the autoconfiguration facilities in the system probe for the device and, if found, enable the software support for it. If a device does not respond at autoconfiguration time, it is not accessible at any time afterwards. To enable a device which did not autoconfigure, the system will have to be rebooted.

The autoconfiguration system is described in autoconf(4). A list of the supported hardware and devices is given below.

# SUPPORTED SYSTEMS

DEC and Compaq have produced a series of the Alpha CPU, some of which are listed below, along with some systems which contain them.

"EV" stands for "Extended VAX" (or "Electro Vlassic") and the number following is a reference to the CMOS process used to make the chips. "LCA" stands for Low Cost Alpha, and "PCA" stands for PC-architecture Alpha.

21064
  EV4 (100-200 MHz, 0.75 micron)

  AlphaPC 64 (EB64)

  Avanti family
    Digital's lower-end PCI-based workstations.

    AlphaStation 200 4/100-166 (Mustang)
    AlphaStation 400 4/166 (Chinet)

  Pelican family
    Low-end TURBOchannel based workstations.

    DEC 3000/300 (150 MHz) (Pelican)
    DEC 3000/300X (175 MHz) (Pelican+)
    DEC 3000/300L (100 MHz) (Pelica)
    DEC 3000/300LX (125 MHz) (Pelica+)

  Sandpiper family
    High-end TURBOchannel based workstations.

    DEC 3000/400 (133 MHz) (Sandpiper)
    DEC 3000/600 (175 MHz) (Sandpiper+)

  Flamingo family
    High-end TURBOchannel based workstations.

    DEC 3000/500 (150 MHz) (Flamingo)
    DEC 3000/500X (200 MHz) (Hot Pink)
    DEC 3000/800 (200 MHz) (Flamingo II)

21064-A
  EV45 (225-333 MHz, 0.50 micron)

  DEC 3000/700 (225 MHz) (Sandpiper45)
  DEC 3000/900 (275 MHz) (Flamingo45)

  Avanti family
    Digital's lower-end PCI-based workstations.

    AlphaStation 200 4/233 (Mustang+)
    AlphaStation 205 4/133-333 (LX3)
    AlphaStation 250 4/300 (M3+)
    AlphaStation 255 4/133-333 (LX3+)
    AlphaStation 300 4/266 (Melmac)
    AlphaStation 400 4/233-300 (Avanti)

21066
  LCA4 (166-233 MHz, 0.75 micron)
  NoName family
    Digital's lowest-end family of PCI-based systems.

    DEC AXPpci33 (NoName)
    Universal Desktop Box AXPpci166MT (UDB/Multia)

  21066 evaluation motherboard (EB66)

21066-A
  LCA45 (233 MHz, 0.50 micron)

  21066-A evaluation motherboard (EB66+)

21068
  LCA4s (66-233 MHz, 0.75 micron)

  Universal Desktop Box AXPpci233MT (UDB/Multia)

21164
  EV5 (250-366 MHz, 0.50 micron)
  Mikasa family
    AlphaServer 1000 5/300 (Pinnacle)
  Noritake family
    AlphaServer 1000A 5/300 (Pinnacle)

    21164 evaluation motherboard (EB164)

21164-A
  EV56 (400-766 MHz, 0.35 micron, BWX)
  Personal Workstation (PWS)
    PWS 433a/433au (Miata)
    PWS 500a/500au (Miata)
    PWS 600a/600au (Miata)
  Mikasa family
    AlphaServer 1000 5/333-500 (Primo)
  Noritake family
    AlphaServer 1000A 5/333-500 (Primo)
    AlphaServer 800 5/333-500 (Corelle)
  EB164 family
    AlphaPC 164 motherboard (EB164)
    AlphaPC 164LX motherboard (EB164)

  DigitalServer 3300 (rebadged AlphaServer 800 for NT)

21164-PC
  PCA56 (400-600 MHz, 0.35 micron, MVI, no L2 cache)

  AlphaPC 164SX motherboard (EB164)

  PWS 466au (Miata)
  PWS 550au (Miata)

21264
  EV6 (450-600 MHz, 0.35 micron)

  APi UP1000 and UP1100; AMD 751-based EV6 systems.

  264DP, XP1000, DS10, DS20 Tsunami-based systems.

21264-A
  EV67 (600-833 MHz, 0.28 micron)

# LIST OF DEVICES

A complete list of available devices is contained within the pages describing the system buses and controllers. For example, a PCI device would be listed in the pci(4) man page. The following buses and controllers list these devices:

eisa(4)
  introduction to EISA bus support
iic(4)
  Inter IC (I2C) bus
isa(4)
  introduction to ISA bus support
onewire(4)
  1-Wire bus
pci(4)
  introduction to PCI bus support
usb(4)
  introduction to Universal Serial Bus support

# SEE ALSO

autoconf(4), config(8)

# HISTORY

The Alpha `intro` first appeared in OpenBSD 2.3.

March 31, 2022 | Debian