NSPHYTER(4) | Device Drivers Manual | NSPHYTER(4)

# NAME

`nsphyter` — National Semiconductor DP83815/DP83843/DP83847 10/100 Ethernet PHY

# SYNOPSIS

`nsphyter* at mii?`

# DESCRIPTION

The `nsphyter` driver supports the National Semiconductor PHYTER DP83843/DP83847 Ethernet PHYs. This driver also supports the integrated PHY on the MacPHYTER DP83815. These PHYs are found on a variety of Ethernet interfaces.

# SEE ALSO

ifmedia(4), intro(4), mii(4), nsphy(4), ifconfig(8)

January 24, 2020 | Debian