ACPISBS(4) | Device Drivers Manual | ACPISBS(4)

# NAME

`acpisbs` — ACPI Smart Battery subsystem

# SYNOPSIS

`acpisbs* at acpi?`

# DESCRIPTION

The `acpisbs` driver supports the ACPI Smart Battery subsystem and provides information about the Smart Battery devices contained within it. Battery status is updated every 30 seconds, as well as in response to events from the subsystem. Battery status can be monitored using sysctl(8) or sensorsd(8).

# SEE ALSO

acpi(4), acpibat(4), intro(4), sensorsd(8), sysctl(8)

# HISTORY

The `acpisbs` driver first appeared in OpenBSD 6.1.

# AUTHORS

The `acpisbs` driver was written by joshua stein <jcs@openbsd.org>.

# CAVEATS

The `acpisbs` driver does not currently support more than one battery.

March 30, 2017 | Debian