IHA(4) | Device Drivers Manual | IHA(4)

# NAME

`iha` — Initio INIC-940/950 based PCI SCSI interface

# SYNOPSIS

`iha* at pci?`

# DESCRIPTION

The `iha` driver supports PCI SCSI host adapters based on the Initio INIC-940, INIC-941 and INIC-950 chips, including the following:

- DTC Domex 3194U Plus
- INI-9090U
- INI-9100U/UW
- Iwill 2935UW

# SEE ALSO

cd(4), ch(4), intro(4), pci(4), scsi(4), sd(4), st(4), uk(4)

http://www.initio.com/

# HISTORY

The `iha` device driver first appeared in OpenBSD 2.9.

# AUTHORS

The `iha` driver was written for OpenBSD by Kenneth R. Westerback, based on a FreeBSD driver by Winston Hung.

# BUGS

`iha` does not currently use tagged command queuing.

January 15, 2015 | Debian