UTVFU(4) | Device Drivers Manual | UTVFU(4)

# NAME

`utvfu` — USB Fushicai USBTV007 audio/video capture device

# SYNOPSIS

`utvfu* at uhub?`
`audio* at utvfu?`
`video* at utvfu?`

# DESCRIPTION

The `utvfu` driver supports USB Audio/Video capture devices based on the Fushicai USBTV007 chip. The following product models are known to work:

- Play X Store Capture
- YXGOOD EasyCAP

If the `utvfu` device attaches successfully, it will attach the audio(4) and video(4) drivers to provide higher-level access.

# SEE ALSO

audio(4), intro(4), usb(4), video(4)

# HISTORY

The `utvfu` driver first appeared in OpenBSD 6.0.

June 4, 2016 | Debian