AUTRI(4) | Device Drivers Manual | AUTRI(4)

# NAME

`autri` — Trident 4DWAVE-DX/NX, SiS 7018, ALi M5451 audio device

# SYNOPSIS

`autri* at pci? flags 0x0000`
`audio* at autri?`
`midi* at autri?`

# DESCRIPTION

The `autri` device driver supports the AC'97 audio controller found in Trident 4DWAVE-DX/NX, SiS 7018 and ALi M5451. `autri` typically has reversed stereo channels. The driver compensates for this, but the compensation can be turned off by setting flags to 0x0001.

# SEE ALSO

ac97(4), audio(4), intro(4), midi(4), pci(4)

# HISTORY

The `autri` device driver appeared in OpenBSD 3.1.

May 31, 2007 | Debian