ET(4) | Device Drivers Manual | ET(4)

# NAME

`et` — Agere/LSI ET1310 10/100/1Gb Ethernet device

# SYNOPSIS

`et* at pci?`
`etphy* at mii?`

# DESCRIPTION

The `et` driver supports PCI Express Ethernet adapters based on the Agere/LSI ET1310 integrated MAC/PHY.

The following media types are supported:

`autoselect`
  Enable autoselection of the media type and options.
`10baseT`
  Set 10Mbps operation.
`100baseTX`
  Set 100Mbps (Fast Ethernet) operation.
`1000baseT`
  Set 1000Mbps (Gigabit Ethernet) operation (some models only).

# SEE ALSO

arp(4), etphy(4), ifmedia(4), intro(4), netintro(4), pci(4), hostname.if(5), ifconfig(8)

# HISTORY

The `et` device driver first appeared in OpenBSD 4.3.

# AUTHORS

The `et` driver was written by Sepherosa Ziehau for DragonFly and ported to OpenBSD by Jonathan Gray <jsg@openbsd.org>.

September 8, 2021 | Debian