SISFB(4) | Device Drivers Manual (loongson) | SISFB(4)

# NAME

`sisfb` — SiS 315 Pro frame buffer

# SYNOPSIS

`sisfb* at pci?`

# DESCRIPTION

The `sisfb` driver supports the SiS 315 Pro frame buffer.

The `sisfb` driver interfaces the frame buffer with the wscons(4) console framework, as a wsdisplay(4) device.

The PMON firmware initializes the frame buffer in a VGA compatible video mode, either with a 640x400 resolution and 8 bits per pixel on Fuloong, or a 1360x768 resolution and 16 bits per pixel on Lynloong. It is currently not possible to change the frame buffer resolution and color depth.

# SEE ALSO

intro(4), pci(4), wscons(4), wsdisplay(4)

March 2, 2010 | Debian