STFPINCTRL(4) | Device Drivers Manual (riscv64) | STFPINCTRL(4)

# NAME

`stfpinctrl` — StarFive JH7100/JH7110 pin configuration

# SYNOPSIS

`stfpinctrl* at fdt?`

# DESCRIPTION

The `stfpinctrl` driver uses pin control data from the device tree to configure pins on the StarFive JH7100/JH7110 SoCs.

# SEE ALSO

intro(4)

# HISTORY

The `stfpinctrl` device driver first appeared in OpenBSD 7.2.

# AUTHORS

The `stfpinctrl` driver was written by Mark Kettenis <kettenis@openbsd.org>.

July 8, 2023 | Debian