DSXRTC(4) | Device Drivers Manual | DSXRTC(4)

# NAME

`dsxrtc` — Maxim DS3231/DS3232 real-time clock

# SYNOPSIS

`dsxrtc* at iic? addr 0x68`

# DESCRIPTION

The `dsxrtc` driver provides support for the Maxim DS3231 and DS3232 real-time clock chips.

# SEE ALSO

iic(4), intro(4)

# HISTORY

The `dsxrtc` driver first appeared in OpenBSD 6.7.

# AUTHORS

The `dsxrtc` driver was written by Mark Kettenis <kettenis@openbsd.org>.

April 25, 2020 | Debian