MLPHY(4) | Device Drivers Manual | MLPHY(4)

# NAME

`mlphy` — MicroLinear 6692 Ethernet PHY

# SYNOPSIS

`mlphy* at mii?`

# DESCRIPTION

The `mlphy` driver supports MicroLinear 6692 10/100 Ethernet PHYs. The MicroLinear PHY only supports 100baseTX operation but can advertise 10baseT operation for a possible companion PHY.

# SEE ALSO

ifmedia(4), intro(4), mii(4), ifconfig(8)

# BUGS

The OUI and device identification of the MicroLinear 6692 PHY are undefined and so `mlphy` only attaches to tl(4) devices using the tlphy(4) as companion PHY.

March 28, 2011 | Debian