DC(4) | Device Drivers Manual | DC(4)

# NAME

`dc` — DEC/Intel 21140/21142/21143/21145 and clones 10/100 Ethernet device

# SYNOPSIS

`dc* at pci?`
`dc* at cardbus?`
`amphy* at mii?`
`bmtphy* at mii?`
`dcphy* at mii?`
`icsphy* at mii?`
`lxtphy* at mii?`
`mtdphy* at mii?`
`nsphy* at mii?`
`nsphyter* at mii?`
`sqphy* at mii?`
`tqphy* at mii?`

# DESCRIPTION

The `dc` driver provides support for several PCI, Mini PCI, and CardBus Fast Ethernet adapters and embedded controllers based on the following chipsets:

- DEC 21140 PCI
- DEC/Intel 21143 PCI and CardBus
- Intel 21145 PCI
- Macronix 98713, 98713A, 98715, 98715A, 98725, 98727 and 98732
- Davicom DM9100, DM9102, and DM9102A
- ASIX Electronics AX88140A and AX88141
- ADMtek AL981 Comet, AN983 Centaur-P and ADM9511/ADM9513 Centaur-II PCI
- ADMtek AN985 Centaur-C CardBus
- Lite-On 82c168 and 82c169 PNIC
- Lite-On/Macronix 82c115 PNIC II
- Xircom X3201-based CardBus

All of these chips have the same general register layout, DMA descriptor format and method of operation. All of the clone chips are based on the 21143 design with various modifications. (The 21140 is an older version of the 21143.) The 21143 itself has support for 10baseT, BNC, AUI, MII and symbol media attachments, 10 and 100Mbps speeds in full or half duplex, and built-in NWAY autonegotiation. The 21143 also offers several receive filter programming options including perfect filtering, inverse perfect filtering and hash table filtering. The 21145 seems to be 10Mbps only and has an additional (unsupported) HomePNA PHY.

Some clone chips duplicate the 21143 fairly closely while others only maintain superficial similarities. Some support only MII media attachments. Others use different receiver filter programming mechanisms. At least one supports only chained DMA descriptors (most support both chained descriptors and contiguously allocated fixed size rings). Some chips (especially the PNIC) also have peculiar bugs. The `dc` driver does its best to provide generalized support for all of these chipsets in order to keep special case code to a minimum.

These chips are used by many vendors, which makes it difficult to provide a complete list of all supported cards. The following NICs are known to work with the `dc` driver at this time:

- Digital DE500-BA 10/100 (21143, non-MII)
- Built-in DE500-BA on DEC Alpha workstations (21143, non-MII)
- Built-in Ethernet on Linksys EtherFast 10/100 Instant GigaDrive (DM9102, MII)
- Kingston KNE100TX (21143, MII)
- D-Link DFE-570TX (21143, MII, quad port)
- NDC SOHOware SFA110A (98713A)
- NDC SOHOware SFA110A Rev B4 (98715AEC-C)
- SVEC PN102-TX (98713)
- CNet Pro120A (98715A or 98713A) and CNet Pro120B (98715)
- Compex RL100-TX (98713 or 98713A)
- Linksys LNE100TX (PNIC 82c168, 82c169)
- NetGear FA310-TX Rev. D1, D2 or D3 (PNIC 82c169)
- Matrox FastNIC 10/100 (PNIC 82c168, 82c169)
- Kingston KNE110TX (PNIC 82c169)
- Linksys LNE100TX v2.0 (PNIC II 82c115)
- Jaton XpressNet (Davicom DM9102)
- Alfa Inc GFC2204 (ASIX AX88140A)
- CNet Pro110B (ASIX AX88140A)
- Linksys LNE100TX v4.x (ADMtek AN983 Centaur-P)
- Xircom CardBus, including RealPort models (Xircom X3201)
- IBM EtherJet 10/100 CardBus (Intel 21143)
- Accton EN1217 (98715) and EN2242 (ADMtek Centaur)
- Mototech ME316 (ADMtek Centaur)
- Conexant LANfinity RS7112 Mini PCI

The `dc` driver supports the following media types:

autoselect
  Enable autoselection of the media type and options. The user can manually override the autoselected mode by adding media options to the hostname.if(5) file.

  Note: the built-in NWAY autonegotiation on the original PNIC 82c168 chip is horribly broken and is not supported by the `dc` driver at this time: the chip will operate in any speed or duplex mode, however these must be set manually. The original 82c168 appears on very early revisions of the Linksys LNE100TX and Matrox FastNIC.

10baseT
  Set 10Mbps operation. The mediaopt option can also be used to enable full-duplex operation. Not specifying full duplex implies half-duplex mode.
100baseTX
  Set 100Mbps (Fast Ethernet) operation. The mediaopt option can also be used to enable full-duplex operation. Not specifying full duplex implies half-duplex mode.

The `dc` driver supports the following media options:

full-duplex
  Force full duplex operation. The interface will operate in half duplex mode if this media option is not specified.

Note that the 100baseTX media type may not be available on certain Intel 21143 adapters which support 10Mbps media attachments only. The Intel 21145 supports 10Mbps half-duplex only.

For more information on configuring this device, see ifconfig(8).

# DIAGNOSTICS

dc0: couldn't map ports/memory
  A fatal initialization error has occurred.
dc0: couldn't map interrupt
  A fatal initialization error has occurred.
dc0: watchdog timeout
  A packet was queued for transmission and a transmit command was issued, however the device failed to acknowledge the transmission before a timeout expired. This can happen if the device is unable to deliver interrupts for some reason, or if there is a problem with the network connection (cable).
dc0: no memory for rx list
  The driver failed to allocate an mbuf for the receiver ring.
dc0: TX underrun -- increasing TX threshold
  The device generated a transmit underrun error while attempting to DMA and transmit a packet. This happens if the host is not able to DMA the packet data into the NIC's FIFO fast enough. The driver will dynamically increase the transmit start threshold so that more data must be DMAed into the FIFO before the NIC will start transmitting it onto the wire.
dc0: TX underrun -- using store and forward mode
  The device continued to generate transmit underruns even after all possible transmit start threshold settings had been tried, so the driver programmed the chip for store and forward mode. In this mode, the NIC will not begin transmission until the entire packet has been transferred into its FIFO memory.

# SEE ALSO

amphy(4), arp(4), bmtphy(4), cardbus(4), dcphy(4), icsphy(4), ifmedia(4), intro(4), lxtphy(4), mtdphy(4), netintro(4), nsphy(4), nsphyter(4), pci(4), sqphy(4), tqphy(4), hostname.if(5), ifconfig(8)

ADMtek AL981 and AL983 data sheets.

ASIX Electronics AX88140A and AX88141 data sheets, https://www.asix.com.tw.

Davicom DM9102 data sheet.

Intel 21143 Hardware Reference Manual, http://developer.intel.com.

Macronix 98713/A, 98715/A and 98725 data sheets, https://www.macronix.com.

Macronix 98713/A and 98715/A app notes, https://www.macronix.com.

# HISTORY

The `dc` device driver first appeared in FreeBSD 4.0. OpenBSD support was added in OpenBSD 2.7.

# AUTHORS

The `dc` driver was written by Bill Paul <wpaul@ee.columbia.edu> and ported to OpenBSD by Aaron Campbell <aaron@openbsd.org>.

# BUGS

The Macronix application notes claim that in order to put the chips in normal operation, the driver must write a certain magic number into the CSR16 register. The numbers are documented in the app notes, but the exact meaning of the bits is not.

The 98713A seems to have a problem with 10Mbps full duplex mode. The transmitter works but the receiver tends to produce many unexplained errors leading to very poor overall performance. The 98715A does not exhibit this problem. All other modes on the 98713A seem to work correctly.

The original 82c168 PNIC chip has built-in NWAY support which is used on certain early Linksys LNE100TX and Matrox FastNIC cards, however it is horribly broken and difficult to use reliably. Consequently, autonegotiation is not currently supported for this chipset: the driver defaults the NIC to 10baseT half duplex, and it's up to the operator to manually select a different mode if necessary. (Later cards use an external MII transceiver to implement NWAY autonegotiation and work correctly.)

The `dc` driver programs 82c168 and 82c169 PNIC chips to use the store and forward setting for the transmit start threshold by default. This is to work around problems with some NIC/PCI bus combinations where the PNIC can transmit corrupt frames when operating at 100Mbps, probably due to PCI DMA burst transfer errors.

The 82c168 and 82c169 PNIC chips also have a receiver bug that sometimes manifests during periods of heavy receive and transmit activity, where the chip will improperly DMA received frames to the host. The chips appear to upload several kilobytes of garbage data along with the received frame data, dirtying several RX buffers instead of just the expected one. The `dc` driver detects this condition and will salvage the frame, however it incurs a serious performance penalty in the process.

The PNIC chips also sometimes generate a transmit underrun error when the driver attempts to download the receiver filter setup frame, which can result in the receive filter being incorrectly programmed. The `dc` driver will watch for this condition and requeue the setup frame until it is transferred successfully.

The ADMtek AL981 chip (and possibly the AN983 as well) has been observed to sometimes wedge on transmit: this appears to happen when the driver queues a sequence of frames which cause it to wrap from the end of the transmit descriptor ring back to the beginning. The `dc` driver attempts to avoid this condition by not queuing any frames past the end of the transmit ring during a single invocation of the `dc_start`() routine. This workaround has a negligible impact on transmit performance.

The `mii_tick`() function does not currently run for ASIX boards, meaning cable disconnects and reconnects can go unnoticed. The AX88140A and AX88141 data sheets indicate that they don't have RX or TX state registers (the bits are reserved). Therefore, we can't seem to reliably detect when the adapter is idle.

The Davicom interfaces require a grossly high PCI latency timer value to function properly. This means when a Davicom adapter is present in the machine, it is given an unfairly high amount of bandwidth on the PCI bus, unnecessarily taking time away from other devices. Therefore, Davicom network cards are not recommended for use with OpenBSD. Be careful; some motherboards have Davicom interfaces built-in.

February 18, 2022 | Debian