MAXTMP(4) | Device Drivers Manual | MAXTMP(4)

# NAME

`maxtmp` — Maxim MAX6642/MAX6690 temperature sensor

# SYNOPSIS

`maxtmp* at iic?`

# DESCRIPTION

The `maxtmp` driver provides support for the Maxim 6642, Maxim 6657, Maxim 6658, Maxim 6659, Maxim 6690, National LM86, National LM89, National LM90, National LM99, and National LM99-1 temperature sensors. The sensor possesses an internal temperature sensor and a link to an external temperature sensor. Both values are made available through the sysctl(8) interface.

# SEE ALSO

iic(4), intro(4), sensorsd(8), sysctl(8)

# HISTORY

The `maxtmp` driver first appeared in OpenBSD 3.9.

# AUTHORS

The `maxtmp` driver was written by Theo de Raadt <deraadt@openbsd.org>.

July 16, 2013 | Debian