UVISOR(4) | Device Drivers Manual | UVISOR(4)

# NAME

`uvisor` — USB Handspring Visor

# SYNOPSIS

`uvisor* at uhub?`
`ucom* at uvisor?`

# DESCRIPTION

The `uvisor` driver provides support for the Handspring Visor, a Palmpilot compatible PDA.

The device is accessed through the ucom(4) driver which makes it behave like a tty(4). The usual Pilot tools can be used to access the Visor.

# SEE ALSO

intro(4), tty(4), ucom(4), uhub(4), usb(4)

# HISTORY

The `uvisor` driver appeared in NetBSD 1.5. OpenBSD support was added in OpenBSD 2.8.

June 26, 2008 | Debian