EX(4) | Device Drivers Manual | EX(4)

# NAME

`ex` — Intel EtherExpress Pro/10 and Pro/10+ Ethernet device

# SYNOPSIS

`ex0 at isa? port 0x320 irq 5`

# DESCRIPTION

The `ex` interface provides access to a 10 Mb/s Ethernet network via the Intel i82595 Ethernet chips. This includes the following models:

Intel EtherExpress Pro/10 ISA
Intel EtherExpress Pro/10+ ISA

# SEE ALSO

arp(4), ifmedia(4), intro(4), isa(4), netintro(4), hostname.if(5), ifconfig(8)

October 23, 2007 | Debian