NVT(4) | Device Drivers Manual | NVT(4)

# NAME

`nvt` — Nuvoton W83795G/ADG temperature, voltage, and fan sensor

# SYNOPSIS

`nvt* at iic?`

# DESCRIPTION

The `nvt` driver provides support for the Nuvoton W83795G and W83795ADG hardware monitors. These devices possess several voltage, temperature and fan speed sensors. Sensor values are made available through the sysctl(8) interface.

# SEE ALSO

iic(4), intro(4), sensorsd(8), sysctl(8)

# HISTORY

The `nvt` driver first appeared in OpenBSD 5.0.

# AUTHORS

The `nvt` driver was written by Mark Kettenis <kettenis@openbsd.org>.

July 16, 2013 | Debian