UOAKRH(4) | Device Drivers Manual | UOAKRH(4)

# NAME

`uoakrh` — Toradex OAK USB temperature and relative humidity sensor

# SYNOPSIS

`uoakrh* at uhidev?`

# DESCRIPTION

The `uoakrh` driver provides support for the Toradex OAK RH. The sensor possesses a collection of sensor values which are made available through the sysctl(8) interface. The relative humidity data unit is "%RH" and the temperature data unit is "degC". The device has a unique serial number, indicated in the description part of the sensor value.

# SEE ALSO

intro(4), uhidev(4), sensorsd(8), sysctl(8)

Toradex Web Page, http://developer.toradex.com/hardware-resources/usb-sensors-and-peripherals.

# HISTORY

The `uoakrh` device driver first appeared in OpenBSD 5.3.

# AUTHORS

The `uoakrh` driver was written by Yojiro UO <yuo@nui.org>.

January 3, 2024 | Debian