ASBTM(4) | Device Drivers Manual | ASBTM(4)

# NAME

`asbtm` — Asus ASB 100 temperature sensor

# SYNOPSIS

`asbtm* at iic?`

# DESCRIPTION

The `asbtm` driver supports the Asus ASB 100 temperature sensor, making its sensor readings available through a sysctl(8) interface.

The driver reads seven voltage (A/D) inputs, three fan inputs, two on-chip temperature sensors and up to two satellite temperature sensors.

# SEE ALSO

iic(4), intro(4), sensorsd(8), sysctl(8)

# AUTHORS

The `asbtm` driver was written by Damien Miller <djm@openbsd.org>.

July 16, 2013 | Debian