NVME(4) | Device Drivers Manual | NVME(4)

# NAME

`nvme` — Non-Volatile Memory Host Controller Interface

# SYNOPSIS

`nvme* at pci?`
`nvme* at aplns? # arm64`

# DESCRIPTION

The `nvme` driver provides support for NVMe, or NVM Express, storage controllers conforming to the Non-Volatile Memory Host Controller Interface specification.

Although the NVMe specification provides its own command set, the `nvme` driver provides access to the storage via a SCSI translation layer.

Sensor values are made available through the hw.sensors sysctl(8) interface.

# SEE ALSO

aplns(4), intro(4), pci(4), scsi(4)

# HISTORY

The `nvme` driver first appeared in OpenBSD 6.0.

# AUTHORS

The `nvme` driver was written by David Gwynne <dlg@openbsd.org>.

September 26, 2024 | Debian