USLCOM(4) | Device Drivers Manual | USLCOM(4)

# NAME

`uslcom` — Silicon Laboratories CP210x based USB serial adapter

# SYNOPSIS

`uslcom* at uhub?`
`ucom* at uslcom?`

# DESCRIPTION

The `uslcom` driver supports Silicon Laboratories CP2101/CP2102/CP2103/CP2104/CP2105/CP2108 based serial adapters.

The CP2101/CP2102/CP2103 devices only support a variety of baud rates up to 921600. CP2104, CP2105 and CP2108 devices support any baud rate up to 2 Mbps.

The following devices should work with the `uslcom` driver:

    Aerocomm Radio
    Argussoft ISP
    Aruba Networks USB-to-UART
    Baltech card reader
    Burnside Telecom Desktop Mobile
    chip45.com Crumb128 module
    Clipsal 5500PCU C-Bus
    Dynastream ANT2USB
    Elan Digital Systems USBscope50
    Elan Digital Systems USBwave12
    Elan Digital Systems USBpulse100
    Elan Digital Systems USBcount50
    Enfora EDG1228
    Gemalto Prox-PU/CU Smartcard Readers
    IRZ MC35pu GSM Terminal
    Jablotron PC-60B
    Juniper SRX 300/320/340/345/550M/1500 USB console
    Lipowsky Baby-JTAG
    Lipowsky Baby-LIN
    Lipowsky HARP-1
    MobiData GPRS Modem
    Pololu USB to Serial
    Ruckus ICX 7150 USB console
    SPORTident BSM7-D-USB
    Tracient RFID
    Track Systems Traqmate
    West Mountain Radio RIGblaster P&P
    West Mountain Radio RIGtalk

# SEE ALSO

tty(4), ucom(4), uhub(4), usb(4)

# HISTORY

The `uslcom` device driver first appeared in OpenBSD 4.0.

# AUTHORS

The `uslcom` driver was written by Jonathan Gray <jsg@openbsd.org>.

December 13, 2021 | Debian