ISLRTC(4) | Device Drivers Manual | ISLRTC(4)

# NAME

`islrtc` — Intersil ISL1208/1218 real-time clock

# SYNOPSIS

`islrtc* at iic? addr 0x6f`

# DESCRIPTION

The `islrtc` driver provides support for the Intersil/Renesas ISL1208 and ISL1218 real-time clock chips.

# SEE ALSO

iic(4), intro(4)

# HISTORY

The `islrtc` driver first appeared in OpenBSD 6.4.

# AUTHORS

The `islrtc` driver was written by Mark Kettenis <kettenis@openbsd.org>.

November 20, 2018 | Debian