ASIO(4) | Device Drivers Manual (sparc64) | ASIO(4)

# NAME

`asio` — SBus Aurora sio2 driver

# SYNOPSIS

`asio* at sbus?`
`com* at asio?`

# DESCRIPTION

The `asio` driver provides support for the Aurora Technologies sio2 serial interface, which is basically a pair of com(4) ports with sbus(4) glue logic.

# SEE ALSO

com(4), intro(4), sbus(4)

# HISTORY

OpenBSD support for `asio` was added in OpenBSD 3.1.

# AUTHORS

The driver was written by Jason Wright <jason@thought.net>.

# BUGS

Only revision 210sj is known to work. Minor work may be necessary for other revisions of this card.

July 16, 2013 | Debian