GSCPM(4) | Device Drivers Manual (i386) | GSCPM(4)

# NAME

`gscpm` — National Semiconductor Geode SC1100 SMI/ACPI module

# SYNOPSIS

`gscpm* at pci?`

# DESCRIPTION

The `gscpm` driver provides support for the National Semiconductor Geode SC1100 System-on-Chip SMI/ACPI module. Only power management timer is supported for now.

# SEE ALSO

intro(4), pci(4)

# HISTORY

The `gscpm` driver first appeared in OpenBSD 3.7.

# AUTHORS

The `gscpm` driver was written by Alexander Yurchenko <grange@openbsd.org>.

July 16, 2013 | Debian