UHA(4) | Device Drivers Manual (i386) | UHA(4)

# NAME

`uha` — Ultrastor SCSI interface

# SYNOPSIS

`uha0 at isa? port 0x330`
`uha1 at isa? port 0x334`
`uha* at eisa?`

# DESCRIPTION

The `uha` driver provides support for the following SCSI adapters:

Ultrastor 14f
Ultrastor 24f
Ultrastor 34f

# SEE ALSO

cd(4), ch(4), eisa(4), intro(4), isa(4), scsi(4), sd(4), st(4), uk(4)

August 14, 2012 | Debian