ICHIIC(4) | Device Drivers Manual | ICHIIC(4)

# NAME

`ichiic` — Intel ICH SMBus controller

# SYNOPSIS

`ichiic* at pci?`
`iic* at ichiic?`

# DESCRIPTION

The `ichiic` driver provides support for the Intel ICH SMBus host interface to be used with the iic(4) framework.

Supported chipsets:

- Intel ICH, ICH2, ICH3, ICH4, ICH4-M, ICH5, ICH5R, ICH6, ICH6-M, ICH6R, ICH7, ICH8, ICH9, ICH10, C-ICH, PCH, 6300ESB and 6321ESB.

# SEE ALSO

iic(4), intro(4), pci(4)

# HISTORY

The `ichiic` driver first appeared in OpenBSD 3.9.

# AUTHORS

The `ichiic` driver was written by Alexander Yurchenko <grange@openbsd.org>.

# BUGS

The driver doesn't support I2C commands with a data buffer size of more than 2 bytes.

July 16, 2013 | Debian