UOAKLUX(4) | Device Drivers Manual | UOAKLUX(4)

# NAME

`uoaklux` — Toradex OAK USB illuminance sensor

# SYNOPSIS

`uoaklux* at uhidev?`

# DESCRIPTION

The `uoaklux` driver provides support for the Toradex OAK LUX. The sensor possesses a collection of sensor values which are made available through the sysctl(8) interface.

The illuminance date unit is "Lux". Because the sensing cycle of the illuminance sensor is faster than the sensor framework update period, the driver keeps maximum/minimum/average values as independent sensors.

The device has a unique serial number, indicated in the description part of the sensor value.

# SEE ALSO

intro(4), uhidev(4), sensorsd(8), sysctl(8)

Toradex Web Page, http://developer.toradex.com/hardware-resources/usb-sensors-and-peripherals.

# HISTORY

The `uoaklux` device driver first appeared in OpenBSD 5.3.

# AUTHORS

The `uoaklux` driver was written by Yojiro UO <yuo@nui.org>.

January 3, 2024 | Debian