AQ(4) | Device Drivers Manual | AQ(4)

# NAME

`aq` — Aquantia AQC1xx 1Gb/2.5Gb/5Gb/10Gb PCIe Ethernet device

# SYNOPSIS

`aq* at pci?`

# DESCRIPTION

The `aq` driver provides support for the Aquantia AQC1xx family of Ethernet adapters.

The `aq` driver supports the following media types:

autoselect
  Enables auto-negotiation for speed and duplex.
100baseTX `mediaopt` full-duplex
  Sets 100Mbps operation.
1000baseT
  Sets 1000Mbps operation.
2500baseT
  Sets 2.5Gbps operation.
5000baseT
  Sets 5Gbps operation.
10GbaseT
  Sets 10Gbps operation.

For more information on configuring this device, see ifconfig(8).

# SEE ALSO

arp(4), ifmedia(4), intro(4), netintro(4), pci(4), hostname.if(5), ifconfig(8)

# HISTORY

The `aq` device driver first appeared in OpenBSD 7.0.

# AUTHORS

The `aq` driver was written by Mike Larkin <mlarkin@openbsd.org> and
Jonathan Matthew <jmatthew@openbsd.org>.

# BUGS

This driver only supports devices using Aquantia firmware version 2.

March 31, 2022 | Debian