JMB(4) | Device Drivers Manual | JMB(4)

# NAME

`jmb` — JMicron JMB36x SATA II and PATA Host Controller

# SYNOPSIS

`jmb* at pci?`
`ahci* at jmb?`
`pciide* at jmb?`

# DESCRIPTION

JMicron JMB36x hardware can provide support for SATA devices using the Advanced Host Controller Interface for Serial ATA, and for PATA devices using PCI IDE controller specification. Since support for both SATA and PATA devices can be enabled on the same PCI device but only one driver per PCI device can be attached, the `jmb` driver acts as a nexus to other drivers that support the SATA and PATA functionality. ahci(4) supports the SATA functionality, and pciide(4) support the PATA functionality on these controllers.

# SEE ALSO

ahci(4), intro(4), pci(4), pciide(4)

# HISTORY

The `jmb` driver first appeared in OpenBSD 4.2.

# AUTHORS

The `jmb` driver was written by David Gwynne <dlg@openbsd.org>.

July 16, 2013 | Debian