MUE(4) | Device Drivers Manual | MUE(4)

# NAME

`mue` — Microchip LAN75xx/LAN78xx 10/100/1Gb USB Ethernet device

# SYNOPSIS

`mue* at uhub?`
`ukphy* at mii?`

# DESCRIPTION

The `mue` driver supports Microchip LAN7500/LAN7505/LAN7515/LAN7850 USB 2.0 Gigabit Ethernet devices and LAN7800/LAN7801 USB 3.0 Gigabit Ethernet devices, including the following:

Microchip EVB-LAN7800LC
Z-TEK ZE582

For more information on configuring this device, see ifconfig(8).

# SEE ALSO

arp(4), ifmedia(4), intro(4), netintro(4), ukphy(4), usb(4), hostname.if(5), ifconfig(8)

# HISTORY

The `mue` device driver first appeared in OpenBSD 6.4.

# AUTHORS

The `mue` driver was written by Kevin Lo <kevlo@openbsd.org>.

September 8, 2021 | Debian