URL(4) | Device Drivers Manual | URL(4)

# NAME

`url` — Realtek RTL8150L 10/100 USB Ethernet device

# SYNOPSIS

`url* at uhub?`
`urlphy* at mii?`

# DESCRIPTION

The `url` driver provides support for USB Ethernet adapters based on the Realtek RTL8150L USB-ether bridge chip.

The `url` driver supports the following adapters:

Abocom RTL8151
BAFO BF-310
Billionton USBKR-100
Compex UE202-B
GreenHouse GH-USB100B
GreenHouse GH-USB100B with HomePNA
Hawking Technology HUF11
Linksys USB100M
Longshine LCS-8138TX
Melco Inc. LUA-KTX
Micronet SP128AR
NetComm NP1010
OQO model 01 (10/100) Ethernet
Repotec RP-USB100-A
SMC 2208USB/ETH
TRENDnet TU-ET100C
Zt USB10/100
ZyXEL Prestige
Z-TEK ZK-R02

For more information on configuring this device, see ifconfig(8).

# DIAGNOSTICS

url0: watchdog timeout
  A packet was queued for transmission and a transmit command was issued, however the device failed to acknowledge the transmission before a timeout expired.
url0: no memory for rx list
  The driver failed to allocate an mbuf for the receiver ring.

# SEE ALSO

arp(4), ifmedia(4), mii(4), netintro(4), uhub(4), usb(4), hostname.if(5), ifconfig(8)

# HISTORY

The `url` device driver first appeared in OpenBSD 3.2.

# AUTHORS

The `url` driver was written by Shingo WATANABE <nabe@nabechan.org>.

July 16, 2013 | Debian