UVSCOM(4) | Device Drivers Manual | UVSCOM(4)

# NAME

`uvscom` — SUNTAC Slipper U VS-10U USB serial adapter

# SYNOPSIS

`uvscom* at uhub?`
`ucom* at uvscom?`

# DESCRIPTION

The `uvscom` driver provides support for the SUNTAC Slipper U VS-10U chip. Slipper U is a PC Card to USB converter for data communication card adapters. It supports DDI Pocket's Air H" C@rd, C@rd H" 64, NTT's P-in, P-in m@ster, and various other data communication card adapters.

The device is accessed through the ucom(4) driver which makes it behave like a tty(4).

# SEE ALSO

tty(4), ucom(4), usb(4)

# HISTORY

The `uvscom` driver first appeared in FreeBSD and later in OpenBSD 3.3.

June 26, 2008 | Debian