UOAKV(4) | Device Drivers Manual | UOAKV(4)

# NAME

`uoakv` — Toradex OAK USB +/-10V 8channel ADC interface

# SYNOPSIS

`uoakv* at uhidev?`

# DESCRIPTION

The `uoakv` driver provides support for the Toradex OAK 10V device. The sensor possesses a collection of sensor values which are made available through the sysctl(8) interface.

The ADC date unit is "VDC"(DC voltage) and the value is signed. Because the Analog-Digital conversion cycle of the device is faster than the sensor framework update cycle, the driver keeps maximum/minimum/average values of each cycle as independent sensors.

The device has a unique serial number, indicated in the description part of the sensor value.

# SEE ALSO

intro(4), uhidev(4), sensorsd(8), sysctl(8)

Toradex Web Page, http://developer.toradex.com/hardware-resources/usb-sensors-and-peripherals.

# HISTORY

The `uoakv` device driver first appeared in OpenBSD 5.3.

# AUTHORS

The `uoakv` driver was written by Yojiro UO <yuo@nui.org>.

January 3, 2024 | Debian