HIRESET(4) | Device Drivers Manual | HIRESET(4)

# NAME

`hireset` — HiSilicon reset controller

# SYNOPSIS

`hireset* at fdt?`

# DESCRIPTION

The `hireset` driver controls the reset signals for integrated components of HiSilicon SoCs.

# SEE ALSO

hiclock(4), intro(4)

# HISTORY

The `hireset` device driver first appeared in OpenBSD 6.4.

# AUTHORS

The `hireset` driver was written by Mark Kettenis <kettenis@openbsd.org>.

August 27, 2018 | Debian