AMAS(4) | Device Drivers Manual | AMAS(4)

# NAME

`amas` — AMD memory address map

# SYNOPSIS

`amas* at pci?`

# DESCRIPTION

The `amas` driver provides read access to the AMD memory map, which describes the location of physical memory.

One instance of this device is shared between all cores on a chip. This device is present on AMD processors of the 0Fh, 10h and 11h family.

The `amas` device can run in either interleaved mode or in non-interleaved mode. In interleaved mode, the physical memory addresses are rotated across each chip. `amas` sits between the CPU cores, the DRAM controller and the HyperTransport bus. When a CPU requests a memory page, `amas` decides if the request is serviced from memory local to the chip, in which case it normalizes the address and passes it on to the dram controller. If the request refers to memory present on a different chip, the request is forwarded to the correct chip using the hypertransport bus.

The `amas` device is configured by the BIOS and kernel startup routines. If multiple instances of this device are available, all should contain the same information.

# SEE ALSO

pci(4)

BIOS and Kernel Developer's Guide for AMD Athlon 64 and AMD Opteron Processors, Publication # 26094, pp. 66–80, February 2006.

BIOS and Kernel Developer's Guide (BKDG) For AMD Family 10h Processors, Publication # 31116, pp. 158–167, March 2008.

BIOS and Kernel Developer's Guide (BKDG) For AMD Family 11h Processors, Publication # 41256, pp. 109–114, July 2008.

# HISTORY

The `amas` driver first appeared in OpenBSD 4.6.

# AUTHORS

The `amas` driver was written by Ariane van der Steldt <ariane@stack.nl>.

July 16, 2013 | Debian