UMCT(4) | Device Drivers Manual | UMCT(4)

# NAME

`umct` — MCT USB-RS232 USB serial adapter

# SYNOPSIS

`umct* at uhub?`
`ucom* at umct?`

# DESCRIPTION

The `umct` driver provides support for MCT USB-to-RS232 Converter and their family products.

The device is accessed through the ucom(4) driver which makes it behave like a tty(4).

# HARDWARE

The `umct` driver supports the following adapters:

Belkin F5U109
Belkin F5U409
D-Link DU-H3SP USB BAY
MCT USB-RS232 Converter 9 pin Model U232-P9
MCT USB-RS232 Converter 25 pin Model U232-P25
Sitecom USB-RS232 Converter

# SEE ALSO

tty(4), ucom(4), uhub(4), usb(4)

# HISTORY

The `umct` driver appeared in OpenBSD 3.2.

January 21, 2019 | Debian