AGTEN(4) | Device Drivers Manual (sparc64) | AGTEN(4)

# NAME

`agten` — Fujitsu AG-10e accelerated 24-bit color frame buffer

# SYNOPSIS

`agten* at sbus?`
`wsdisplay* at agten?`

# DESCRIPTION

The Fujitsu AG-10e is a two-slot SBus color frame buffer, with graphics acceleration and overlay capabilities, including hardware OpenGL processing.

The `agten` driver interfaces the frame buffer with the wscons(4) console framework. It does not provide direct device driver entry points but makes its functions available via the internal wsdisplay(4) interface.

# SEE ALSO

intro(4), sbus(4), wscons(4), wsdisplay(4)

# CAVEATS

This driver does not support any acceleration features at the moment, and drives the card in PROM-compatible, 8 bit, mode only.

March 31, 2008 | Debian