UTS(4) | Device Drivers Manual | UTS(4)

# NAME

`uts` — USB touchscreen support

# SYNOPSIS

`uts* at uhub?`
`wsmouse* at uts? mux 0`

# DESCRIPTION

The `uts` driver provides support for USB touchscreens. Access to the touchscreen is provided through the wscons(4) framework.

Touching the screen will emulate mouse button 0 being pressed.

The touchscreen sensor is poorly aligned, therefore xtsscale(1) should be used to provide calibration results to the `uts` driver.

The `uts` driver works with the following touchscreens and panels:

- Gunze USB Touch Panel
- Hantouch
- LG L1510SF LCD Monitor
- Origin AE X15e HTPC case with 7" LCD

# SEE ALSO

xtsscale(1), uhub(4), usb(4), wscons(4), wsmouse(4)

# HISTORY

The `uts` driver first appeared in OpenBSD 4.2.

# AUTHORS

The `uts` driver was written by Robert Nagy <robert@openbsd.org>.

July 16, 2013 | Debian