OCTXCTL(4) | Device Drivers Manual (octeon) | OCTXCTL(4)

# NAME

`octxctl` — OCTEON USB3 controller bridge

# SYNOPSIS

`octxctl* at fdt?`
`xhci* at octxctl?`

# DESCRIPTION

The `octxctl` driver provides support for the OCTEON USB3 controller bridge. The bridge connects the system's I/O bus and a USB3 controller.

# SEE ALSO

xhci(4)

# HISTORY

The `octxctl` driver first appeared in OpenBSD 6.2.

August 1, 2017 | Debian