XE(4) | Device Drivers Manual | XE(4)

# NAME

`xe` — Xircom-based 16-bit PCMCIA 10/100 Ethernet device

# SYNOPSIS

`xe* at pcmcia?`
`icsphy* at mii?`

# DESCRIPTION

The `xe` interface provides access to a 10/100 Mb/s Ethernet network via a Xircom Ethernet card. The Ethernet cards known to be supported by the `xe` interface are:

Xircom Realport
Xircom CE3

However, most 16-bit Xircom Ethernet cards should work.

# SEE ALSO

arp(4), icsphy(4), ifmedia(4), intro(4), netintro(4), pcmcia(4), hostname.if(5), ifconfig(8)

# HISTORY

The `xe` driver appeared in OpenBSD 2.5.

May 31, 2007 | Debian