MONGOOSE(4) | Device Drivers Manual (hppa) | MONGOOSE(4)

# NAME

`mongoose` — EISA Bus adapter

# SYNOPSIS

`mongoose0 at mainbus?`
`eisa* at mongoose?`

# DESCRIPTION

Provides an interface from the CPU-memory bus to EISA and ISA devices. Two variations exist providing the same functionality based on Intel i82350 or Texas Instruments chips. Depending on the model the bus clock is either 25 MHz or 33 MHz.

# SEE ALSO

eisa(4), intro(4)

# HISTORY

The `mongoose` driver appeared in OpenBSD 2.6.

# BUGS

Has some.

May 31, 2007 | Debian