OCTPCIE(4) | Device Drivers Manual (octeon) | OCTPCIE(4)

# NAME

`octpcie` — OCTEON PCIe controller

# SYNOPSIS

`octpcie* at iobus?`
`pci* at octpcie?`

# DESCRIPTION

The `octpcie` driver provides support for the OCTEON PCIe controller found on OCTEON II and III. It provides a host interface to the pci(4) bus.

# DIAGNOSTICS

octpcie0 port N: link timeout
  The PCIe link did not establish. This happens if the PCIe slot is empty.
octpcie0 port N: reset timeout
  The PCIe port failed to reset. This can happen if the PCIe port has not been wired.

# SEE ALSO

intro(4), pci(4)

# HISTORY

The `octpcie` driver first appeared in OpenBSD 6.6.

October 7, 2019 | Debian