STGE(4) | Device Drivers Manual | STGE(4)

# NAME

`stge` — Sundance/Tamarack TC9021 1Gb Ethernet device

# SYNOPSIS

`stge* at pci?`
`eephy* at mii?`
`gentbi* at mii?`
`ipgphy* at mii?`

# DESCRIPTION

The `stge` device driver supports the Sundance/Tamarack TC9021 Gigabit Ethernet chip.

The Sundance/Tamarack TC9021 chip is found on adapters such as the following:

- Allied Telesis CentreCOM LA1000-PCI-T
- Antares Microsystems TC9021
- Asus NX1101
- D-Link DGE-550T

It uses an external PHY or an external 10-bit interface.

The `stge` driver supports IPv4 receive IP/TCP/UDP checksum offload and VLAN tag insertion and stripping.

# SEE ALSO

arp(4), eephy(4), gentbi(4), ifmedia(4), intro(4), ipgphy(4), mii(4), netintro(4), pci(4), hostname.if(5), ifconfig(8)

# HISTORY

The `stge` driver first appeared in OpenBSD 3.1.

# AUTHORS

The `stge` driver was written by Jason R. Thorpe <thorpej@netbsd.org>.

September 8, 2021 | Debian