XGE(4) | Device Drivers Manual | XGE(4)

# NAME

`xge` — Neterion Xframe/Xframe II 10Gb Ethernet device

# SYNOPSIS

`xge* at pci?`

# DESCRIPTION

The `xge` device driver provides support for various NICs based on the Neterion Xframe and Xframe II controller chips, including the following:

- Fujitsu PRIMEQUEST 10GBASE-SR LAN Card (Xframe II)
- Hitachi PCI-X 10 Gigabit Ethernet Adapter (Xframe II)
- HP AB287A 10 Gigabit Ethernet Adapter (Xframe)
- IBM 10GbE SR Server Adapter (Xframe II)
- IBM 10 Gb Ethernet-LR PCI-X 2.0 DDR Adapter (Xframe II)
- IBM 10 Gb Ethernet-SR PCI-X 2.0 DDR Adapter (Xframe II)
- Neterion/S2io Xframe (Xframe)
- Neterion Xframe II (Xframe II)
- Neterion Xframe II Sun Fire (Xframe II)
- Neterion Xframe E (Xframe II)
- SGI 10 Gigabit Ethernet Network Adapter (Xframe)

The Xframe and Xframe II support IPv4 transmit/receive IP/TCP/UDP checksum offload and VLAN tag insertion and stripping.

# SEE ALSO

arp(4), ifmedia(4), netintro(4), pci(4), ifconfig(8)

# HISTORY

The `xge` driver first appeared in OpenBSD 4.0.

# AUTHORS

The `xge` driver was written by Anders Magnusson <ragge@ludd.luth.se> and ported to OpenBSD by Brad Smith <brad@openbsd.org>.

July 16, 2013 | Debian