BRSWPHY(4) | Device Drivers Manual | BRSWPHY(4)

# NAME

`brswphy` — Broadcom BCM53xx 10/100/1000TX Ethernet PHY

# SYNOPSIS

`brswphy* at mii?`

# DESCRIPTION

The `brswphy` driver supports Broadcom BCM53115 10/100/1000TX Ethernet PHY interfaces found on some of the octeon models.

# SEE ALSO

ifmedia(4), intro(4), mii(4), ifconfig(8)

# HISTORY

The `brswphy` driver first appeared in OpenBSD 5.6.

# AUTHORS

The `brswphy` driver was written by Paul Irofti <paul@irofti.net>.

April 6, 2020 | Debian