SHPCIC(4) | Device Drivers Manual (landisk) | SHPCIC(4)

# NAME

`shpcic` — landisk SuperH PCI-Host Bridge

# SYNOPSIS

`shpcic* at mainbus?`
`pci0 at shpcic?`

# DESCRIPTION

The `shpcic` driver provides support for the landisk on-board PCI bus. This device is largely transparent and provides no user accessible entry points.

# SEE ALSO

mainbus(4), pci(4)

# HISTORY

The `shpcic` driver first appeared in OpenBSD 4.1.

September 19, 2010 | Debian